Exercise 15: Reading A Pushbutton With The Basic Stamp

Work Activities 2 through 4 in Chapter 3 of the Parallax Manual What’s a Microcontroller?, pg 75-88.   Some of the materials in these activities have been covered in earlier exercises, which should make the time required to complete these activities somewhat shorter.  When you have completed the activities, answer the following questions.

Questions:
1.  What is the difference between sending and receiving HIGH and LOW signals

using the BASIC Stamp?

2.  What does “normally open” mean in regards to a pushbutton?

3.  What kind of code blocks can be used for making decisions based on the value

of one or more pushbuttons?

4. What does the HOME formatter do in the statement DEBUG HOME?

5.  Explain how to modify ReadPushbuttonState.bs2 on page 77 so that it reads the

pushbutton every second instead of every ¼ second.










